{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Results"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Results","index":0,"n_rows":13,"n_cols":65,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,0,1,64],[2,51,2,64],[2,0,2,8],[2,9,2,20],[2,21,2,38],[2,39,2,42],[2,43,2,50]]}
["ACEA RDE Monitoring Platform - 3rd package"]
[]
["Identification of PEMS TEST FAMILY (MS-OEM-X-Y)",null,null,null,null,null,null,null,null,"Technical Criteria for PEMS TEST FAMILY",null,null,null,null,null,null,null,null,null,null,null,"PEMS test results",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Declared maximum RDE values",null,null,null,"Criteria for PEMS TEST Vehicle Selection",null,null,null,null,null,null,null," Justification for PEMS tests"]
["PEMS TEST FAMILY","TAA code","MF code","emission type","Make","commercial name"," type","variant","version","WVTA","propulsion type","fuel type","combustion process","No of cyl.","conf. cyl. block","displ.","fuel inject.","cooling sys.","air supply","type&sequ. aftertreatment","EGR","MAW_MNOx,d,t","MAW_MCO,d,t","MAW_MPN,d,t ","MAW_MNOx,d,u ","MAW_MCO,d,u ","MAW_MPN,d,u","SPF_MNOx,d,t","SPF _MCO,d,t","SPF _MPN,d,t ","SPF _MNOx,d,u ","SPF _MCO,d,u","SPF _MPN,d,u ","M_NOx,d,t","M_CO,d,t","M_PN,d,t ","M_NOx,d,u ","M_CO,d,u","M_PN,d,u ","Complete RDE trip: NOx","Complete RDE trip: PN","Urban RDE trip: NOx","Urban RDE trip: PN","fuel","P to M","transmiss.","prop.","displ.","No. of aftertr. compo.","tot. amount of ET","test driven by","fuel","PMR H","PMR L","transm.","xWD","eng.vol.","aftertreat.","cold test","warm test","No. of ET","No. of tests","TS test share","div. eng. vol.","comments"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"[cm³]",null,null,null,null,null,"[mg/km]","[mg/km]","[#/km]","[mg/km]","[mg/km]","[#/km]","[mg/km]","[mg/km]","[#/km]","[mg/km]","[mg/km]","[#/km]","[mg/km]","[mg/km]","[#/km]","[mg/km]","[mg/km]","[#/km]","[mg/km]","[#/km]","[mg/km]","[#/km]",null,"[W/kg]"]
["13-SJA-4VV8D-0000",13,"SJA","e13*715/2007*2016/646ZD*6740*00","Bentley","Bentayga Diesel","4V-715-Y","AC*Y*",1,"e11*2007/46*3609*01","ICE","Diesel","4-stroke",8,"V",3956,"DI","water","3-turbo","NOC+SCRF","y",48,281,"n.a. (*)",33,584,"n.a. (*)","-","-","n.a. (*)","-","-","n.a. (*)","-","-","-","-","-","-","126","600000000000","126","600000000000","Diesel",121,"Auto","AWD",3956,"NOC+SCRF",1,"TS","x","x",null,"x","x","x","x","x",null,1,2,0.5,0,"(*) PN test procedure not yet available"]
["13-SJA-4VV8D-0000",13,"SJA","e13*715/2007*2016/646ZD*6740*00","Bentley","Bentayga Diesel","4V-715-Y","AC*Y*",2,"e11*2007/46*3609*01","ICE","Diesel","4-stroke",8,"V",3956,"DI","water","3-turbo","NOC+SCRF","y",48,281,"n.a. (*)",33,584,"n.a. (*)","-","-","n.a. (*)","-","-","n.a. (*)","-","-","-","-","-","-","126","600000000000","126","600000000000","Diesel",121,"Auto","AWD",3956,"NOC+SCRF",1,"TS","x","x",null,"x","x","x","x","x",null,1,2,0.5,0,"(*) PN test procedure not yet available"]
["13-SJA-4VV8-0000",13,"SJA","e13*715/2007*2017/1221W*6796*01","Bentley","Bentayga V8","4VD","AD*X*",1,"e11*2007/46*3609*03","ICE","Gasoline","4-stroke",8,"V",3996,"DI","water","2-turbo","TWC","n",11,127,"n.a. (*)",23,18,"n.a. (*)","-","-","n.a. (*)","-","-","n.a. (*)","-","-","-","-","-","-","126","600000000000","126","600000000000","Gasoline",162,"Auto","AWD",3996,"TWC",1,"TS","x","x",null,"x","x","x","x","x",null,1,2,0.5,0,"(*) PN test procedure not yet available"]
["13-SJA-4VV8-0000",13,"SJA","e13*715/2007*2017/1221W*6796*01","Bentley","Bentayga V8","4VD","AD*X*",2,"e11*2007/46*3609*03","ICE","Gasoline","4-stroke",8,"V",3996,"DI","water","2-turbo","TWC","n",11,127,"n.a. (*)",23,18,"n.a. (*)","-","-","n.a. (*)","-","-","n.a. (*)","-","-","-","-","-","-","126","600000000000","126","600000000000","Gasoline",162,"Auto","AWD",3996,"TWC",1,"TS","x","x",null,"x","x","x","x","x",null,1,2,0.5,0,"(*) PN test procedure not yet available"]
["13-SCB-3SA-0000",13,"SCB","e13*715/2007*2017/1221ZD*6792*01","Bentley","Continental GT","3SA","C*AZAA",1,"e13*2007/46*0634*01","ICE","Gasoline","4-stroke",12,"W",5950,"DI+MPI","water","2-turbo","TWC","n",12,73,"n.a. (*)",null,null,"n.a. (*)","-","-","n.a. (*)","-","-","n.a. (*)","-","-","-","-","-","-","126","600000000000","126","600000000000","Gasoline",162,"Auto","AWD",5950,"TWC",1,"TS","x","x",null,"x","x","x","x","x",null,1,2,0.5,0,"(*) PN test procedure not yet available"]
["13-SCB-3SA-0000",13,"SCB","e13*715/2007*2017/1221ZD*6792*01","Bentley","Continental GT","3SA","C*AZAA",2,"e13*2007/46*0634*01","ICE","Gasoline","4-stroke",12,"W",5950,"DI+MPI","water","2-turbo","TWC","n",12,73,"n.a. (*)",null,null,"n.a. (*)","-","-","n.a. (*)","-","-","n.a. (*)","-","-","-","-","-","-","126","600000000000","126","600000000000","Gasoline",162,"Auto","AWD",5950,"TWC",1,"TS","x","x",null,"x","x","x","x","x",null,1,2,0.5,0,"(*) PN test procedure not yet available"]
["11-SCB-3YV8-0000",11,"SCB","e11*715/2007*2017/1347AD*9749*00","Bentley","Mulsanne","3Y","A?A4?Z",1,"e11*2007/46*3609???","ICE","Gasoline","4-stroke",8,"V",6752,"DI","water","2-turbo","TWC","n",43.5,0,"n.a. (*)",32.9,0,"n.a. (*)","-","-","n.a. (*)","-","-","n.a. (*)","-","-","-","-","-","-","126","600000000000","126","600000000000","Gasoline",null,"Auto","AWD",6752,"TWC",1,"GC","x","x",null,"x","x","x","x","x",null,1,2,0.5,0,"(*) PN test procedure not yet available"]
["11-SCB-3YV8-0000",11,"SCB","e11*715/2007*2017/1347AD*9749*00","Bentley","Mulsanne","3Y","A?A4?Z",2,"e11*2007/46*3609???","ICE","Gasoline","4-stroke",8,"V",6752,"DI","water","2-turbo","TWC","n",43.5,0,"n.a. (*)",32.9,0,"n.a. (*)","-","-","n.a. (*)","-","-","n.a. (*)","-","-","-","-","-","-","126","600000000000","126","600000000000","Gasoline",null,"Auto","AWD",6752,"TWC",1,"GC","x","x",null,"x","x","x","x","x",null,1,2,0.5,0,"(*) PN test procedure not yet available"]